The distance between two measurement areas is 9 mm!
The first MA cannot be measured. The data starts from 2nd MA. 
Both 2um*2um and 4*4 um images are exported. The roughness is calculated from 4*4 um image.