The distance between two measurement areas is 4.5 mm! The last MA is on Pt
The first MA cannot be measured. The data starts from 2nd MA. 
4*4 um image is exported. The roughness is calculated accordingly.